|  |
| --- |
|  |
|  | /\* outgoing CMD Bytes after \*/ |
|  | CMD\_SYSTEM\_QUERY = 0x0, 0 |
|  | CMD\_SYSTEM\_GET\_ID = 0x1, 0 |
|  | CMD\_SYSTEM\_SET\_ID = 0x2, 32 |
|  | CMD\_SYSTEM\_GET\_OFFSETS = 0x3, 0 |
|  | CMD\_SYSTEM\_SET\_OFFSET = 0x4, 3 |
|  | CMD\_SYSTEM\_GET\_GRIDSZ = 0x5, 0 |
|  | CMD\_SYSTEM\_SET\_GRIDSZ = 0x6, 2 |
|  | CMD\_SYSTEM\_GET\_ADDR = 0x7, 0 |
|  | CMD\_SYSTEM\_SET\_ADDR = 0x8, 2 |
|  | CMD\_SYSTEM\_GET\_VERSION = 0xF, 0 |
|  |  |
|  | /\* incoming CMD Bytes In \*/ |
|  | CMD\_SYSTEM\_QUERY\_RESPONSE = 0x0, 2 |
|  | CMD\_SYSTEM\_ID = 0x1, 32 |
|  | CMD\_SYSTEM\_GRID\_OFFSET = 0x2, 3 |
|  | CMD\_SYSTEM\_GRIDSZ = 0x3, 2 |
|  | CMD\_SYSTEM\_ADDR = 0x4, 2 |
|  | CMD\_SYSTEM\_VERSION = 0xF, 8 |
|  |  |
|  | /\* outgoing CMD Bytes after \*/ |
|  | CMD\_LED\_OFF = 0x0, 2 |
|  | CMD\_LED\_ON = 0x1, 2 |
|  | CMD\_LED\_ALL\_OFF = 0x2, 0 |
|  | CMD\_LED\_ALL\_ON = 0x3, 0 |
|  | CMD\_LED\_MAP = 0x4, 10 |
|  | CMD\_LED\_ROW = 0x5, 3 |
|  | CMD\_LED\_COLUMN = 0x6, 3 |
|  | CMD\_LED\_INTENSITY = 0x7, 1 |
|  | CMD\_LED\_LEVEL\_SET = 0x8, 3 |
|  | CMD\_LED\_LEVEL\_ALL = 0x9, 1 |
|  | CMD\_LED\_LEVEL\_MAP = 0xA, 34 |
|  | CMD\_LED\_LEVEL\_ROW = 0xB, 6 |
|  | CMD\_LED\_LEVEL\_COLUMN = 0xC, 6 |
|  |  |
|  | /\* incoming CMD Bytes In \*/ |
|  | CMD\_KEY\_UP = 0x0, 2 |
|  | CMD\_KEY\_DOWN = 0x1, 2 |